# Led blinking code for raspberry:-

import machine

import time

led = machine.Pin('LED', machine.Pin.OUT) # Initialize the LED pin

print('Hello')

while True:

led.value(1) # Turn the LED on

time.sleep(1) # Wait for 1 second

led.value(0) # Turn the LED off

time.sleep(0.4) # Wait for 0.4 seconds

